流程说明

运行在：APP/Boot loader 内流程一致：

PC->BMS: 5AA5 XXXX(row number)+row data : send one row to BMS

BMS->PC: 5AA5 02XX XX(row number)+CRC : program one row ok

loop until the whole file has been sent to BMS

PC->BMS: 5AA5 3344+CRC :enter boot loader mode

BMS->PC: 5AA5 00AA 55+CRC :enter boot loader mode ok

PC->BMS: 5AA5 FEEF+CRC :start to erase app flash

BMS->PC: 5AA5 01AA 55+CRC : erase app flash ok

BMS->PC: 5AA5 03XX XX(row number)+CRC :receive the last row

PC->BMS: 5AA5 FAAF+CRC :jump to APP